­­

Unpack Inputs

Check for entry/exits of vehicles

Check for vehicles that are fully charged

Driving

Check for changes in tariff

**Recalculate charge rate**

Assign charge rate

Y

+5 mins

N

Event?

Determine whether extra charging is needed